Appendix 1: Summary of Relevant Jordanian Ambient Air Quality Standards (No. 1140/2206)

|  |  |  |  |
| --- | --- | --- | --- |
| Air Pollutant | Average Time | Maximum Allowable Concentration in theAmbient Air | Number of AllowedExceedences |
| Carbon Monoxide (CO) | 1 hr | 26 mg/kg | 3 times within a given month in one year |
| 8 hr | 9 mg/kg | 3 times within a given month in one year |
| Nitrogen Dioxide (NO2) | 1 hr | 0.21 mg/kg | 3 times within a given month in one year |
| 24 hr | 0.08 mg/kg | 3 times within a given month in one year |
| 1 Yr | 0.05 mg/kg | -- |
| Sulfur Dioxide (SO2) | 1 hr | 0.30 mg/kg | 3 times within a given month in one year |
| 24 hr | 0.14 mg/kg | Once a year |
| 1 Yr | 0.04 mg/kg | -- |